MeshForge candidate review
Verification token
Draft for human review. This candidate remains review required. Report approval permits document handoff only; it does not approve the model for production or publication.
Evidence date: 2026-10-10 | Report generated: 2026-10-17 | Profile: Preview
Source and candidate
	Controlled source
[image: ]
Full silhouette, neutral light, isolated object.
	Generated candidate
[image: ]
Recognizable silhouette and inset, with softened material detail and no separable body or inset roles.


Recorded measurements
	Measure
	Recorded value

	Runtime
	80.76 sec

	Triangles
	35,796

	Components
	1 logical / 222 raw

	Topology edges
	0 logical / 5,040 raw

	Status
	Review required


Review decision
The basic form survives, including the inset. After attribute splits are welded, the candidate is one logical manifold component. Its softened form, fused material role, and missing semantic labels still make it a visual blockout.
Decision pending. Check: Does the candidate preserve the hexagonal body, shallow top inset, and visible thickness without inventing an unstable underside?
Provenance: benchmark summary and paired assets copied into this package with SHA256 checksums. Measurements are reproduced from the recorded benchmark; no new generation or verifier run is claimed.
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